Search processing.org:

Reference for Processing (BETA) version 0135+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Class | Serial
Name | ### read()
Examples |
    // Example by Tom Igoe

    import processing.serial.*;

    Serial myPort;  // The serial port

    void setup() {
      // List all the available serial ports
      println(Serial.list());
      // I know that the first port in the serial list on my mac
      // is always my  Keyspan adaptor, so I open Serial.list()[0].
      // Open whatever port is the one you're using.
      myPort = new Serial(this, Serial.list()[0], 9600);
    }

    void draw() {
      while (myPort.available() > 0) {
        int inByte = myPort.read();
        println(inByte);
      }
    }
Description | Returns a number between 0 and 255 for the next byte that's waiting in the buffer. Returns -1 if there is no byte, although this should be avoided by first cheacking available() to see if data is available.
Syntax |
    serial.read()
Parameters |
serial | any variable of type Serial
Usage | Web & Application

Updated on December 20, 2005 02:03:00pm PST